include:
  - hamview-broker.yaml

receiver:
  type: companion
  conf:
    port: /dev/ttyUSB0
    baud: 115200

    # Trace performs periodic tracing
    trace:
      interval: 5m
      links:
        # Via NL-NTD-Omni
        #   - PI-AIR-VSR RP3
        - [0x78, 0xbf, 0x78]
        #   - Didam Omni
        - [0x78, 0x41, 0x78]
        #   - Didam Yagi 1
        - [0x78, 0x9a, 0x78]
